--->> Valid only if the camera is using any version of firmware v8.xx.xx <<---

Follow the instrucions below to update your camera:

1. Make sure the camera battery is fully charged.
2. Turn on the camera.
3. Connect the camera to the computer using a USB cable.
4. From file manager, open the internal memory on the camera
5. Copy the update file (.fuf file extension) from your computer to the folder "doupdate" on the camera.
6. Once you drop the .fuf file in the doupdate folder, the update process starts automatically.
During the update, the camera is unavailable.
7. When the update is completed, the camera restarts automatically.

Important Note: Do not remove the USB cable until the update is completed.


Note: Further information and guides on how to update your camera can be found on the following link: https://flir.custhelp.com/app/answers/detail/a_id/6100