**FLIR Breach PTQ136 Firmware Update**

**Objective:**  
To update the FLIR Breach PTQ136.

**Update: OTS\_PTQ233.bin**

1. Be sure your camera has a fully charged battery, over 95% indicator.
2. Plug the unit into a computer using a USB-C cable (included with unit).
3. Open File Explorer/Windows Explorer and copy the firmware file “OTS\_PTQ233.bin” to the root directory of the unit (USB drive).
4. Unplug the USB cable from the computer and the screen on the unit will show “Uploading OTS software”.
5. A menu will appear asking to update Yes/No. Select "Yes" and update will start.
6. Firmware will install and unit will self-restart.